Sample number – 2 bytes

Internal temperature – 2 bytes

Pressure – 2 bytes

External temperature – 2 bytes

Humidity – 2 bytes

Seconds – 2 bytes

Gps fix – 1 byte

Longitude – 4 bytes

Latitude – 4 bytes

Altitude – 2 bytes

Acceleration x – 2 bytes

Acceleration y – 2 bytes

Acceleration z – 2 bytes

Gyro x – 2 bytes

Gyro y – 2 bytes

Gyro z – 2 bytes

Heading – 2 bytes

Pitch – 2 bytes

Roll – 2 bytes